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1.0 Purpose

1.1 To define the operating procedures for the Laurell WB400B spin coater.

2.0 Scope

2.1 Outline the process qualification requirements for the CVD process chambers.
2.2 Define all CVD process recipe parameters.

2.3 Describe documentation for Process control and Lot Records.

3.0 Associated Materials
3.1 Wafer.
3.2 Material for spin coating.

3.3 Solvent.

3.4 Cleanroom wipes.
4.0 Safety
4.1 Do not open the lid once the spin coating process has begun. 

5.0 Procedures
5.1 Choose a pre-spin coat program on the control panel or input a setting.

5.2 On the control panel located above the spin coater unit, press the vacuum button.
5.3 Place wafer onto centering tool.

5.4 Place the centering tool with the wafer around the spin chuck. The centering tool designed to fit around the spin chuck.
5.5 Apply material to spin onto the wafer and Close lid or, dispense material from the opening on the lid.
5.6 To begin the spin process, press the start button.

5.7 When the spin cycle has completed, press the vacuum button to release the vacuum.

5.8 Remove wafer from the spin chuck.

6.0 Clean up
6.1 Clean up the coater using the appropriate solvent. Wipe using cleanroom wipes until the coater is completely clean.



























SPECIFICATION FORMAT:�
�
�
EQUIPMENT MANUFACTURER:�
Laurell Technologies Corporation�
�
EQUIPMENT MODEL:�
WS400B�
�
FDC ASSIGNED TOOL ID NUMBER:�
A.S.U. Property # 4027564�
�
APPLICATION PROGRAM(S) AND REVISION:�
Microsoft Word 2003�
�
�
�
�

































	Arizona State University – Flexible Display Center confidential information.  Hardcopy may not be current document.
	Page 3 of 3



